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Aerofoam-NBR: The highly flexible insulation material for preventing condensation and energy losses

Reliable technical properties 
Dubai, July 15th 2011 − With Aerofoam-NBR Hira Ind. is now presenting its new insulation material for refrigeration, ventilation and air-conditioning applications with very good technical properties. After the successful launch of Aerofoam-XPE in 2010, Aerofoam-NBR comes to enlarge the wide product range of Hira Ind. consisting of ducting accessories, Diamond pipe supports, self-adhesive tapes and moulded and extruded rubber products. The new product already complies with most of the British Standards (BS) and American Standards (ASTM) which are required for pipe insulation from nitrile butadiene rubber (NBR).
Aerofoam-NBR is a highly flexible, closed-cell insulation material which provides installations with reliable protection against condensation and energy losses. Due to its technical properties – high resistance to water vapour diffusion (µ-value), low thermal conductivity (λ-value) – the new Aerofoam-NBR ensures long-term condensation control. It thus also increases the energy efficiency of the in​stallation in comparison to other elastomeric insulation materials and to other types of materials used for the same scope. Fur​thermore, the balanced price-performance ratio makes this material a par​ticularly economical energy-saving solution. 
The benefits of the Aerofoam-NBR at a glance: 

· Fire classification according to BS 476 parts 6 & 7
· Very good resistance to water vapour diffusion: μ ≥ 7.000

· Low thermal conductivity value: λ=0.035 W/m°C at 20°C
· Wide range of applications: refrigeration, HVAC air ducts, water pipelines, water tanks, under slab, raised floors, AHU's, FCU's, etc.
· Great form stability and ease of use 

· Complete range of tubes and sheets (also in self-adhesive, continuous-length and pre-cut versions, on demand)
· Noise reduction properties
The new Aerofoam-NBR has a high resistance to diffusion and low thermal conductivity. Therefore, with this material the risks of moisture penetration are lower than with other insulation materials. The resistance to diffusion is built up continuously – cell by cell – throughout the entire material thickness. The cell walls are ‘sealed’ during production allowing a very high resistance to water vapour diffusion to be achieved. 
Hira Ind. has begun its production of elastomeric pipe insulation since February 2011. Now the complete Aerofoam-NBR range is available: 

· tubes – with thicknesses of 6 mm, 9 mm, 13 mm, 19 mm, 25 mm and 32 mm and with a diameter range between 6 mm and 89 mm;
· rolls – normal or self-adhesive – with thicknesses of 6 mm, 9 mm, 13 mm, 16 mm, 19 mm, 25 mm, 32 mm, 40 mm and 50 mm;

· sheets – with thicknesses of 10 mm, 15 mm, 20 mm and 25 mm.
On demand we are able to offer also sheets or rolls with different aluminium-based foils and also pre-cut tubes. Accessories like self-adhesive rubber tape, adhesive, cleaner and paint against UV are also available.

Specification clauses and the technical calculation programme have already been created for the new product.

Aerofoam-NBR made by Hira Ind. is the local brand in the field of flexible technical insulation which targets fast regional growth through quality and commitment to the customers. The company decided to begin the production of Aerofoam-NBR from the wish to offer a complete solutions package to the customers in the HVAC field. The further products’ development will follow the market needs, will integrate cost-effective and environmental friendly production technologies and will focus on product quality and high service level.

Aerofoam-NBR tubes and sheets are used to insulate pipes and air-ducts. The products prevent condensation, absorb noise and vibrations and protect in​stallations against energy losses. 
Hira Industries LLC is a productive company based in Dubai – UAE, which manufactures rubber and polyethylene products, tapes, ventilation accessories and the Diamond pipe supports. With branches in Oman, Kuwait, Qatar, Saudi Arabia, India and soon in Africa, employing more than 500 people and having a turnover of about 45 mil. USD, Hira Ind. LLC is the only company from the GCC region that can provide both XPE and NBR pipe insulation. The company is ISO certified and follows all the required quality standards for producing the Aerofoam articles. Further information on the company can be found at www.rhira.com and further information on the pipe insulation can be found at www.aerofoam.ae. 
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Caption: 

Aerofoam-NBR and Aerofoam-XLPE have complete delivery programmes 
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